**Basic ALL-IN-ONE Wash and Wax:**

* **For pricing call, text, email, or complete and submit a customer questionnaire**

Includes:

1. Wash entire RV including roof, sides, slide outs and slide out awnings
2. Wash tires, rims, apply silicone tire dressing
3. Cleaning of Awnings

Heavily soiled or stained awnings and/or roofs may incur an additional charge (no guarantee on all spot removal).

**Deluxe Wash and High-Grade Polymer Spray Wax:**

* **Price: An additional $100.00 over Basic Detail**

Includes:

1. “Basic ALL-IN-ONE Wash and Wax” treatment, with the addition of:
	1. Treatment of slide out seals
	2. Application of Protective treatment for rubber roofs
	3. rinse for Spot-free finish
	4. Apply Polymer Spray Wax

Heavily soiled or stained awnings and/or roofs will be an additional charge (no guarantee on spot removal).

**Platinum Wash and Wax:**

* **Price: Estimated upon evaluation and Inspection**

Includes:

1. “Basic ALL-IN-ONE Wash and Wax” treatment, with the addition of:
	1. Treatment of slide out seals
	2. Spray wax fiberglass roof; Application of Protective treatment for rubber roofs
	3. Deionized rinse for Spot-free finish
	4. Cleaning of Awnings
	5. Application of high-quality paste wax
	6. Application of Rain-X to all windows including the windshield

Heavily soiled or stained awnings and/or roofs may incur an additional charge (no guarantee on all spot removal).

**Gel coated RVs are not recommended for this option. This task is very labor intensive and not cost effective for the consumer. A Waxed and polished gel coated RV will only return to its oxidated state within approximately six (6) months**.

**Additional Services Pricing List**

**A/C Preventative maintenance.** Cleaning of the condenser coils and evaporator coils from sediment and debris. Combing of the cooling fins. Vacuuming and removal of debris from the a/c components. Removing and washing of the a/c filters. Inspection of the a/c duct to ensure proper sealing (resealing if necessary). Make efficiency enhancements and recommendations.

One A/C 100.00

Two A/C’s 175.00

Three A/C’s 225.00

**Hot Water Heater maintenance**. Flushing of the hot water heater tank. Removal of the anode. Inspection of the interior of the hot water tank for any signs of corrosion, or damage from any form of degradation. Washing of any sediment from the tank. Inspection of the heating element for any damages, or signs of degradation to warrant replacement. Visual inspection of all electrical and propane components for damage or debris. Replace anode if warranted.

100.00 which includes the replacement anode if needed.

**Black tank / Grey Tank Pressure Washing.** Cleaning and removal of debris and Struvite from the interior walls of the Black and Grey Tanks. Insertion through the exit port of the Black and Grey tank an endoscopy pressure washer nozzle and hose.

Many times, tank sensors do not function properly due to debris becoming lodged upon the sensor probe within the tank. This debris dries and is difficult to remove, which renders the tank sensor inoperable.

As well, a common problem that can occur within black tanks, is what’s referred to as a poop pile (poop mountain, etc.) this can create a problem with drainage and create an obstruction. Not to mention the odor associated with this issue.

100.00 for the cleaning of both grey and black tanks as well as galley tank if associated with the same exit port.

50.00 additional charge if cleaning of an additional tank located at a different exit port.